PepperDash Essentials v1.0.x Installation

1. Download PepperDash Essentials.zip from Portal
   1. Open Zip file
   2. Using FTP client, copy Program01 folder contents (.cpz file) to processor’s Program01 folder
2. Load program without configuration using “progload -p:1” in console. This will create the file structure on the processor
3. Download any needed touchpanel files from Portal
   1. Load vtz to touchpanels
   2. Load iPad core3 project to processor using Toolbox
   3. Load each panel type’s .sgd file to \NVRAM\Program1\sgd folder. TSW 560, 760, 1060, and/or iPad.
4. Download configurationFile.json from Portal
   1. Load configurationFile.json to processor’s \NVRAM\Program1 folder
5. Reset program using “progreset -p:1” in console.